# Manual FED Entries / Test Results

## Revision 2

### Operator Name:

noel

### Time Stamp:

2006-05-04, 15:20:47

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK | Pgood led (ds18) faulty.

Manufacturers Reference No. | Value
--- | ---
PCB_No | 0306
Batch_No | 7569

2D Barcode Value
30201300000336

Opto RX | Serial Number
--- | ---
1 | 3x0495
2 | 3x0494
3 | 3x0497
4 | 3x0496
5 | 3x0498
6 | 3x0499
7 | 3x0501
8 | 380349

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK | Fails ident on U9_2 and U12_1 could be false errors REF NOEL FOUND 120 OHM WORKS R1199 R1201 | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/336/BS_Files/BS_Ident_File_336_Revision2.txt
Boundary Scan 'Inter' Test | OK | Fails ident on U9_2 and U12_1 could be false errors | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/336/BS_Files/BS_Inter_File_336_Revision2.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 1

### Operator Name:

Ivan

### Time Stamp:

2006-03-29, 13:22:57

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK | Pgood led (ds18) faulty.

Manufacturers Reference No. | Value
--- | ---
PCB_No | 0306
Batch_No | 7569

2D Barcode Value
30201300000336

Opto RX | Serial Number
--- | ---
1 | 3x0495
2 | 3x0494
3 | 3x0497
4 | 3x0496
5 | 3x0498
6 | 3x0499
7 | 3x0501
8 | 380349

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | Fail | Fails ident on U9_2 and U12_1 could be false errors | /
Boundary Scan 'Inter' Test | Fail | Fails ident on U9_2 and U12_1 could be false errors | /

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 0

### Operator Name:

noel

### Time Stamp:

2006-01-26, 18:56:13

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Unattempted
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | Fail | Pgood led (ds18) faulty.

Manufacturers Reference No. | Value
--- | ---
PCB_No | 0306
Batch_No | 7569

2D Barcode Value
30201300000336

Opto RX | Serial Number
--- | ---
1 | 3x0495
2 | 3x0494
3 | 3x0497
4 | 3x0496
5 | 3x0498
6 | 3x0499
7 | 3x0501
8 | 380349

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | Unattempted |  | /
Boundary Scan 'Inter' Test | Unattempted |  | /

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Unattempted |
Power On In System Test Crate | Unattempted |
Program VME PROM | Unattempted |
Reboot PC3205, Check Flashing LEDs | Unattempted |