# FED Analog Test Results

## Test 13

### Operator Name:

noel

### Time Stamp:

2006-05-25, 16:18:10

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 12

### Operator Name:

noel

### Time Stamp:

2006-04-25, 12:24:04

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 11

### Operator Name:

noel

### Time Stamp:

2006-04-25, 12:14:07

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 10

### Operator Name:

noel

### Time Stamp:

2006-04-25, 12:06:00

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 9

### Operator Name:

noel

### Time Stamp:

2006-04-25, 11:19:15

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 8

### Operator Name:

noel

### Time Stamp:

2006-04-25, 11:12:38

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 7

### Operator Name:

noel

### Time Stamp:

2006-04-21, 15:40:48

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 6

### Operator Name:

noel

### Time Stamp:

2006-04-18, 12:46:36

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 5

### Operator Name:

noel

### Time Stamp:

2006-04-18, 12:25:49

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 4

### Operator Name:

noel

### Time Stamp:

2006-04-18, 12:16:06

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC values are not monotonic | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 3

### Operator Name:

noel

### Time Stamp:

2006-04-18, 12:10:20

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 2

### Operator Name:

noel

### Time Stamp:

2006-04-18, 12:00:52

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 1

### Operator Name:

noel

### Time Stamp:

2006-04-13, 15:05:36

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 0

### Operator Name:

noel

### Time Stamp:

2006-04-13, 13:07:09

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | ADC value is stuck | ADC value is stuck | ADC value is stuck
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK