# FED Digital Test Results

## Test 0

### Operator Name:

bill

### Time Stamp:

2005-11-24, 13:10:53

### Firmware Version Test Results:

FPGA Name | Test Result | Firmware Version Found | Comment
--- | --- | --- | ---
VME FPGA | Pass | 2100031D | OK
BE FPGA | Pass | 2200036D | OK
FE FPGA 1 | Pass | 23000319 | OK
FE FPGA 2 | Pass | 23000319 | OK
FE FPGA 3 | Pass | 23000319 | OK
FE FPGA 4 | Pass | 23000319 | OK
FE FPGA 5 | Pass | 23000319 | OK
FE FPGA 6 | Pass | 23000319 | OK
FE FPGA 7 | Pass | 23000319 | OK
FE FPGA 8 | Pass | 23000319 | OK

### Voltage Test Results:

Voltage Level | Test Result | Measured Voltage | Comment
--- | --- | --- | ---
2.5V | Pass | 2.486980V | OK
3.3V | Pass | 3.179690V | OK
5V | Pass | 4.895830V | OK
12V | Pass | 11.812500V | OK
Core (1.5V) | Pass | 1.488280V | OK
Supply (3.3V) | Pass | 3.179690V | OK

### Temperature Test Results:

FE Unit | Chip | Test Result | Measured Temperature | Comment
--- | --- | --- | --- | ---
FE Unit 1 | LM82 | Pass | 37degC | OK
| FPGA | Pass | 31degC | OK
FE Unit 2 | LM82 | Pass | 43degC | OK
| FPGA | Pass | 30degC | OK
FE Unit 3 | LM82 | Pass | 44degC | OK
| FPGA | Pass | 32degC | OK
FE Unit 4 | LM82 | Pass | 45degC | OK
| FPGA | Pass | 32degC | OK
FE Unit 5 | LM82 | Pass | 48degC | OK
| FPGA | Pass | 33degC | OK
FE Unit 6 | LM82 | Pass | 48degC | OK
| FPGA | Pass | 33degC | OK
FE Unit 7 | LM82 | Pass | 50degC | OK
| FPGA | Pass | 33degC | OK
FE Unit 8 | LM82 | Pass | 48degC | OK
| FPGA | Pass | 33degC | OK
BE FPGA | LM82 | Pass | 30degC | OK
| FPGA | Pass | 39degC | OK
VME FPGA | LM82 | Pass | 26degC | OK
| FPGA | Pass | 25degC | OK

### Trim DAC and Opto Rx HW Access Test Results:

FE Unit | Channel | Test Result | Trim DAC Comment | Opto Rx Comment
--- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK
| 2 | Pass | OK | OK
| 3 | Pass | OK | OK
| 4 | Pass | OK | OK
| 5 | Pass | OK | OK
| 6 | Pass | OK | OK
| 7 | Pass | OK | OK
| 8 | Pass | OK | OK
| 9 | Pass | OK | OK
| 10 | Pass | OK | OK
| 11 | Pass | OK | OK
| 12 | Pass | OK | OK
2 | 1 | Pass | OK | OK
| 2 | Pass | OK | OK
| 3 | Pass | OK | OK
| 4 | Pass | OK | OK
| 5 | Pass | OK | OK
| 6 | Pass | OK | OK
| 7 | Pass | OK | OK
| 8 | Pass | OK | OK
| 9 | Pass | OK | OK
| 10 | Pass | OK | OK
| 11 | Pass | OK | OK
| 12 | Pass | OK | OK
3 | 1 | Pass | OK | OK
| 2 | Pass | OK | OK
| 3 | Pass | OK | OK
| 4 | Pass | OK | OK
| 5 | Pass | OK | OK
| 6 | Pass | OK | OK
| 7 | Pass | OK | OK
| 8 | Pass | OK | OK
| 9 | Pass | OK | OK
| 10 | Pass | OK | OK
| 11 | Pass | OK | OK
| 12 | Pass | OK | OK
4 | 1 | Pass | OK | OK
| 2 | Pass | OK | OK
| 3 | Pass | OK | OK
| 4 | Pass | OK | OK
| 5 | Pass | OK | OK
| 6 | Pass | OK | OK
| 7 | Pass | OK | OK
| 8 | Pass | OK | OK
| 9 | Pass | OK | OK
| 10 | Pass | OK | OK
| 11 | Pass | OK | OK
| 12 | Pass | OK | OK
5 | 1 | Pass | OK | OK
| 2 | Pass | OK | OK
| 3 | Pass | OK | OK
| 4 | Pass | OK | OK
| 5 | Pass | OK | OK
| 6 | Pass | OK | OK
| 7 | Pass | OK | OK
| 8 | Pass | OK | OK
| 9 | Pass | OK | OK
| 10 | Pass | OK | OK
| 11 | Pass | OK | OK
| 12 | Pass | OK | OK
6 | 1 | Pass | OK | OK
| 2 | Pass | OK | OK
| 3 | Pass | OK | OK
| 4 | Pass | OK | OK
| 5 | Pass | OK | OK
| 6 | Pass | OK | OK
| 7 | Pass | OK | OK
| 8 | Pass | OK | OK
| 9 | Pass | OK | OK
| 10 | Pass | OK | OK
| 11 | Pass | OK | OK
| 12 | Pass | OK | OK
7 | 1 | Pass | OK | OK
| 2 | Pass | OK | OK
| 3 | Pass | OK | OK
| 4 | Pass | OK | OK
| 5 | Pass | OK | OK
| 6 | Pass | OK | OK
| 7 | Pass | OK | OK
| 8 | Pass | OK | OK
| 9 | Pass | OK | OK
| 10 | Pass | OK | OK
| 11 | Pass | OK | OK
| 12 | Pass | OK | OK
8 | 1 | Pass | OK | OK
| 2 | Pass | OK | OK
| 3 | Pass | OK | OK
| 4 | Pass | OK | OK
| 5 | Pass | OK | OK
| 6 | Pass | OK | OK
| 7 | Pass | OK | OK
| 8 | Pass | OK | OK
| 9 | Pass | OK | OK
| 10 | Pass | OK | OK
| 11 | Pass | OK | OK
| 12 | Pass | OK | OK

### Serial EPROM Test Results:

Test Result | Pass
Initialisation Status | Remove Eprom Write Protection: OK
Byte Status | All OK