# FED Analog Test Results

## Test 9

### Operator Name:

noel

### Time Stamp:

2006-08-04, 17:18:02

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 8

### Operator Name:

noel

### Time Stamp:

2006-05-02, 16:33:29

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 7

### Operator Name:

noel

### Time Stamp:

2006-05-02, 16:24:11

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | Unsaturated ADC region too small - Opto Rx problem? | ADC value is stuck high (1023) | Gradient of linear region out of acceptable range
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 6

### Operator Name:

noel

### Time Stamp:

2006-05-02, 15:14:42

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | Unsaturated ADC region too small - Opto Rx problem? | ADC value is stuck high (1023) | Gradient of linear region out of acceptable range
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 5

### Operator Name:

noel

### Time Stamp:

2006-04-05, 16:42:43

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | ADC value is stuck | ADC value is stuck high (1023) | Gradient of linear region out of acceptable range
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 4

### Operator Name:

noel

### Time Stamp:

2006-02-23, 11:51:35

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | Unsaturated ADC region too small - Opto Rx problem? | ADC value is stuck high (1023) | Gradient of linear region out of acceptable range
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | ADC values are not monotonic | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 3

### Operator Name:

noel

### Time Stamp:

2006-02-23, 11:45:14

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | ADC value is stuck | ADC value is stuck high (1023) | Gradient of linear region out of acceptable range
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 2

### Operator Name:

noel

### Time Stamp:

2006-02-23, 11:36:43

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | Unsaturated ADC region too small - Opto Rx problem? | ADC value is stuck high (1023) | Gradient of linear region out of acceptable range
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 1

### Operator Name:

noel

### Time Stamp:

2006-02-22, 17:00:52

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | Gradient of linear region out of acceptable range
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 0

### Operator Name:

noel

### Time Stamp:

2006-02-22, 16:52:12

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | ADC value is stuck | ADC value is stuck high (1023) | Gradient of linear region out of acceptable range
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK