# FED Analog Test Results

## Test 7

### Operator Name:

noel

### Time Stamp:

2006-05-10, 16:34:14

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 6

### Operator Name:

noel

### Time Stamp:

2006-04-24, 14:01:35

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Fail | Linear region contains outlying points | OK | OK
| 2 | Fail | Linear region contains outlying points | OK | OK
| 3 | Fail | Linear region contains outlying points | OK | OK
| 4 | Fail | Linear region contains outlying points | OK | OK
| 5 | Fail | Linear region contains outlying points | OK | OK
| 6 | Fail | Linear region contains outlying points | OK | OK
| 7 | Fail | ADC values are not monotonic | OK | OK
| 8 | Fail | Linear region contains outlying points | OK | OK
| 9 | Fail | Linear region contains outlying points | OK | OK
| 10 | Fail | Linear region contains outlying points | OK | OK
| 11 | Fail | Linear region contains outlying points | OK | OK
| 12 | Fail | Linear region contains outlying points | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 5

### Operator Name:

noel

### Time Stamp:

2006-04-24, 13:55:10

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Fail | ADC values are not monotonic | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 4

### Operator Name:

noel

### Time Stamp:

2006-04-24, 13:31:36

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Fail | Unsaturated ADC region too small - Opto Rx problem? | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Fail | ADC values are not monotonic | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 3

### Operator Name:

noel

### Time Stamp:

2006-04-24, 13:23:20

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Fail | ADC values are not monotonic | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 2

### Operator Name:

noel

### Time Stamp:

2006-04-21, 17:50:56

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Fail | ADC values are not monotonic | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 1

### Operator Name:

noel

### Time Stamp:

2006-04-07, 15:28:55

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Fail | ADC values are not monotonic | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 0

### Operator Name:

noel

### Time Stamp:

2006-04-07, 14:49:50

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Fail | ADC values are not monotonic | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK