# FED Analog Test Results

## Test 13

### Operator Name:

noel

### Time Stamp:

2006-07-31, 17:20:24

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 12

### Operator Name:

noel

### Time Stamp:

2006-07-31, 17:01:22

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Fail | Linear region contains outlying points | Gradient of linear region out of acceptable range | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 11

### Operator Name:

noel

### Time Stamp:

2006-07-31, 16:52:30

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 10

### Operator Name:

noel

### Time Stamp:

2006-07-31, 16:46:58

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 9

### Operator Name:

noel

### Time Stamp:

2006-07-31, 16:30:42

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 8

### Operator Name:

noel

### Time Stamp:

2006-07-31, 15:36:18

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 7

### Operator Name:

noel

### Time Stamp:

2006-07-31, 15:27:58

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 6

### Operator Name:

noel

### Time Stamp:

2006-07-31, 15:22:08

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 5

### Operator Name:

noel

### Time Stamp:

2006-07-31, 12:01:13

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 4

### Operator Name:

noel

### Time Stamp:

2006-07-28, 18:04:36

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 3

### Operator Name:

noel

### Time Stamp:

2006-07-28, 17:02:52

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 2

### Operator Name:

noel

### Time Stamp:

2006-07-28, 16:03:32

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 1

### Operator Name:

noel

### Time Stamp:

2006-07-28, 15:33:15

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Fail | ADC value is stuck | Gradient of linear region out of acceptable range | ADC value is stuck
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Fail | ADC values are not monotonic | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 0

### Operator Name:

noel

### Time Stamp:

2006-05-31, 20:12:27

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 2 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 3 | Fail | ADC value is stuck | ADC values are not monotonic | ADC value is stuck
| 4 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 5 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 6 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 7 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 8 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 9 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 10 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 11 | Fail | ADC values are not monotonic | ADC value is stuck | ADC value is stuck
| 12 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
2 | 1 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 2 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 3 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 4 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 5 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 6 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 7 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 8 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 9 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 10 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 11 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 12 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
3 | 1 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 2 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 3 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 4 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 5 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 6 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 7 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 8 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 9 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 10 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 11 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 12 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
4 | 1 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 2 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 3 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 4 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 5 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 6 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 7 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 8 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 9 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 10 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 11 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 12 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
5 | 1 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 2 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 3 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 4 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 5 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 6 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 7 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 8 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 9 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 10 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 11 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 12 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
6 | 1 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 2 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 3 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 4 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 5 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 6 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 7 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 8 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 9 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 10 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 11 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 12 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
7 | 1 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 2 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 3 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 4 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 5 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 6 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 7 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 8 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 9 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 10 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 11 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 12 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
8 | 1 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 2 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 3 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 4 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 5 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 6 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 7 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 8 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 9 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 10 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 11 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)
| 12 | Fail | OK | ADC value is stuck | ADC value is stuck low (0)