# Manual FED Entries / Test Results

## Revision 2

### Operator Name:

bill

### Time Stamp:

2005-07-27, 16:04:07

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK | TR9 reversed - now repaired.
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK | Incorectly mounted TR9 - repaired. U129 replaced.

Manufacturers Reference No. | Value
--- | ---
PCB_No | 001
Batch_No | 7266

2D Barcode Value
30201300000045

Opto RX | Serial Number
--- | ---
1 | 380499
2 | 380501
3 | 380503
4 | 380505
5 | 380500
6 | 380502
7 | 380504
8 | 380506

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/045/BS_Files/BS_Ident_File_045_Revision2.txt
Boundary Scan 'Inter' Test | OK | SLINK_LSF2 fails for first 3 runs - bad connection on loopback card. | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/045/BS_Files/BS_Inter_File_045_Revision2.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 1

### Operator Name:

bill

### Time Stamp:

2005-07-27, 14:02:04

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK | TR9 reversed - now repaired.
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK | Incorectly mounted TR9 - repaired.

Manufacturers Reference No. | Value
--- | ---
PCB_No | 001
Batch_No | 7266

2D Barcode Value
30201300000045

Opto RX | Serial Number
--- | ---
1 | 380499
2 | 380501
3 | 380503
4 | 380505
5 | 380500
6 | 380502
7 | 380504
8 | 380506

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/045/BS_Files/BS_Ident_File_045_Revision1.txt
Boundary Scan 'Inter' Test | Fail | SLINK_LSF2 fails for first 3 runs. | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/045/BS_Files/BS_Inter_File_045_Revision1.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 0

### Operator Name:

phil

### Time Stamp:

2005-07-26, 14:55:04

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | Fail | Incorectly mounted TR9

Manufacturers Reference No. | Value
--- | ---
PCB_No | 001
Batch_No | 7266

2D Barcode Value
00000000000000

Opto RX | Serial Number
--- | ---
1 | 380499
2 | 380501
3 | 380503
4 | 380505
5 | 380500
6 | 380502
7 | 380504
8 | 380506

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | Unattempted |  | /
Boundary Scan 'Inter' Test | Unattempted |  | /

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Unattempted |
Power On In System Test Crate | Unattempted |
Program VME PROM | Unattempted |
Reboot PC3205, Check Flashing LEDs | Unattempted |