# FED Analog Test Results

## Test 25

### Operator Name:

noel

### Time Stamp:

2006-02-17, 20:26:27

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 24

### Operator Name:

Ivan

### Time Stamp:

2006-02-09, 14:02:46

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 23

### Operator Name:

Ivan

### Time Stamp:

2006-02-09, 13:41:56

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 22

### Operator Name:

Ivan

### Time Stamp:

2006-02-09, 13:35:26

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 21

### Operator Name:

Ivan

### Time Stamp:

2006-02-09, 13:16:47

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 20

### Operator Name:

noel

### Time Stamp:

2006-02-07, 13:59:14

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 19

### Operator Name:

noel

### Time Stamp:

2006-02-07, 12:21:21

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 18

### Operator Name:

noel

### Time Stamp:

2006-02-06, 14:03:55

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Fail | ADC values are not monotonic | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 17

### Operator Name:

noel

### Time Stamp:

2006-02-06, 12:03:24

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 16

### Operator Name:

noel

### Time Stamp:

2006-02-03, 13:03:58

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 15

### Operator Name:

noel

### Time Stamp:

2006-01-26, 15:47:52

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 14

### Operator Name:

noel

### Time Stamp:

2006-01-25, 20:51:13

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 13

### Operator Name:

noel

### Time Stamp:

2006-01-25, 14:53:47

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 12

### Operator Name:

noel

### Time Stamp:

2006-01-25, 14:23:53

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 11

### Operator Name:

noel

### Time Stamp:

2006-01-25, 14:04:38

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 10

### Operator Name:

noel

### Time Stamp:

2006-01-25, 13:57:05

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 9

### Operator Name:

noel

### Time Stamp:

2006-01-25, 13:50:19

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 8

### Operator Name:

noel

### Time Stamp:

2006-01-25, 13:43:08

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 7

### Operator Name:

noel

### Time Stamp:

2006-01-25, 13:36:34

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Fail | ADC values are not monotonic | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 6

### Operator Name:

noel

### Time Stamp:

2006-01-25, 11:28:25

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Fail | Linear region contains outlying points | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 5

### Operator Name:

noel

### Time Stamp:

2006-01-25, 11:06:30

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 4

### Operator Name:

noel

### Time Stamp:

2006-01-25, 10:55:35

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 3

### Operator Name:

noel

### Time Stamp:

2006-01-18, 17:08:40

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 2

### Operator Name:

noel

### Time Stamp:

2006-01-16, 13:14:55

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 1

### Operator Name:

noel

### Time Stamp:

2006-01-13, 17:17:27

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK

## Test 0

### Operator Name:

noel

### Time Stamp:

2006-01-13, 17:07:07

### Trim DAC and Opto Rx FED Channel Test Results:

FE Unit | Channel | Test Result | Trim DAC Offset Comment | Opto Rx Input Offset Comment | Opto Rx Output Offset Comment
--- | --- | --- | --- | --- | ---
1 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
2 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
3 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
4 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
5 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
6 | 1 | Fail | ADC value is stuck high (1023) | ADC value is stuck high (1023) | ADC value is stuck
| 2 | Fail | ADC value is stuck | OK | OK
| 3 | Fail | ADC value is stuck | OK | OK
| 4 | Fail | ADC value is stuck | OK | OK
| 5 | Fail | ADC value is stuck | OK | OK
| 6 | Fail | ADC value is stuck | OK | OK
| 7 | Fail | ADC value is stuck | OK | OK
| 8 | Fail | ADC value is stuck | OK | OK
| 9 | Fail | ADC value is stuck | OK | OK
| 10 | Fail | ADC value is stuck | OK | OK
| 11 | Fail | ADC value is stuck | OK | OK
| 12 | Fail | ADC value is stuck | OK | OK
7 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK
8 | 1 | Pass | OK | OK | OK
| 2 | Pass | OK | OK | OK
| 3 | Pass | OK | OK | OK
| 4 | Pass | OK | OK | OK
| 5 | Pass | OK | OK | OK
| 6 | Pass | OK | OK | OK
| 7 | Pass | OK | OK | OK
| 8 | Pass | OK | OK | OK
| 9 | Pass | OK | OK | OK
| 10 | Pass | OK | OK | OK
| 11 | Pass | OK | OK | OK
| 12 | Pass | OK | OK | OK