# Manual FED Entries / Test Results

## Revision 2

### Operator Name:

noel

### Time Stamp:

2006-04-25, 17:00:01

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK | SOLDER SPLASH POSSIBLE PCB U/S

Manufacturers Reference No. | Value
--- | ---
PCB_No | 0416
Batch_No | 7572

2D Barcode Value
30201300000488

Opto RX | Serial Number
--- | ---
1 | 380518
2 | 380517
3 | 380520
4 | 380519
5 | 380521
6 | 380522
7 | 380524
8 | 380523

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/488/BS_Files/BS_Ident_File_488_Revision2.txt
Boundary Scan 'Inter' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/488/BS_Files/BS_Inter_File_488_Revision2.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 1

### Operator Name:

noel

### Time Stamp:

2006-04-25, 10:00:53

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | Fail | SOLDER SPLASH POSSIBLE PCB U/S

Manufacturers Reference No. | Value
--- | ---
PCB_No | 0416
Batch_No | 7572

2D Barcode Value
30201300000488

Opto RX | Serial Number
--- | ---
1 | 380518
2 | 380517
3 | 380520
4 | 380519
5 | 380521
6 | 380522
7 | 380524
8 | 380523

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/488/BS_Files/BS_Ident_File_488_Revision1.txt
Boundary Scan 'Inter' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/488/BS_Files/BS_Inter_File_488_Revision1.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Unattempted |
Power On In System Test Crate | Unattempted |
Program VME PROM | Unattempted |
Reboot PC3205, Check Flashing LEDs | Unattempted |

## Revision 0

### Operator Name:

noel

### Time Stamp:

2006-04-18, 15:46:34

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | Fail | SOLDER SPLASH POSSIBLE PCB U/S

Manufacturers Reference No. | Value
--- | ---
PCB_No | 0416
Batch_No | 7572

2D Barcode Value
30201300000488

Opto RX | Serial Number
--- | ---
1 | 380518
2 | 380517
3 | 380520
4 | 380519
5 | 380521
6 | 380522
7 | 380524
8 | 380523

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | Unattempted |  | /
Boundary Scan 'Inter' Test | Unattempted |  | /

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Unattempted |
Power On In System Test Crate | Unattempted |
Program VME PROM | Unattempted |
Reboot PC3205, Check Flashing LEDs | Unattempted |