# Manual FED Entries / Test Results

## Revision 3

### Operator Name:

bill

### Time Stamp:

2005-09-08, 12:18:42

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 034
Batch_No | 7266

2D Barcode Value
30201300000071

Opto RX | Serial Number
--- | ---
1 | 390640
2 | 390642
3 | 390643
4 | 390645
5 | 390647
6 | 390641
7 | 390644
8 | 390646

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/071/BS_Files/BS_Ident_File_071_Revision3.txt
Boundary Scan 'Inter' Test | OK | RN8_7 BRIDGE. REFLOWED | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/071/BS_Files/BS_Inter_File_071_Revision3.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 2

### Operator Name:

bill

### Time Stamp:

2005-08-30, 12:50:22

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 034
Batch_No | 7266

2D Barcode Value
30201300000071

Opto RX | Serial Number
--- | ---
1 | 390640
2 | 390642
3 | 390643
4 | 390645
5 | 390647
6 | 390641
7 | 390644
8 | 390646

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/071/BS_Files/BS_Ident_File_071_Revision2.txt
Boundary Scan 'Inter' Test | OK | RN8_7 BRIDGE. REFLOWED | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/071/BS_Files/BS_Inter_File_071_Revision2.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | Fail |
Reboot PC3205, Check Flashing LEDs | Unattempted |

## Revision 1

### Operator Name:

bill

### Time Stamp:

2005-08-30, 03:06:17

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Unattempted |
Fit Front Panel Serial No. Label | Unattempted |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 034
Batch_No | 7266

2D Barcode Value
30201300000071

Opto RX | Serial Number
--- | ---
1 | 390640
2 | 390642
3 | 390643
4 | 390645
5 | 390647
6 | 390641
7 | 390644
8 | 390646

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/071/BS_Files/BS_Ident_File_071_Revision1.txt
Boundary Scan 'Inter' Test | OK | RN8_7 BRIDGE. REFLOWED | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/071/BS_Files/BS_Inter_File_071_Revision1.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | Fail |
Reboot PC3205, Check Flashing LEDs | Unattempted |

## Revision 0

### Operator Name:

bill

### Time Stamp:

2005-08-30, 03:03:47

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Unattempted |
Fit Front Panel Serial No. Label | Unattempted |
Enter Manufacturer Reference Numbers | Unattempted
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Unattempted
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No |
Batch_No |

2D Barcode Value
30201300000071

Opto RX | Serial Number
--- | ---
1 |
2 |
3 |
4 |
5 |
6 |
7 |
8 |

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/071/BS_Files/BS_Ident_File_071_Revision0.txt
Boundary Scan 'Inter' Test | OK | RN8_7 BRIDGE. REFLOWED | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/071/BS_Files/BS_Inter_File_071_Revision0.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | Fail |
Reboot PC3205, Check Flashing LEDs | Unattempted |