# Manual FED Entries / Test Results

## Revision 3

### Operator Name:

Ivan

### Time Stamp:

2005-09-08, 14:51:54

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 030
Batch_No | 7266

2D Barcode Value
30201300000057

Opto RX | Serial Number
--- | ---
1 | 380212
2 | 380211
3 | 380214
4 | 380213
5 | 380216
6 | 380218
7 | 380215
8 | 380217

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/057/BS_Files/BS_Ident_File_057_Revision3.txt
Boundary Scan 'Inter' Test | OK | Boundary Scan Clock TCK Frequency: 2MHz | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/057/BS_Files/BS_Inter_File_057_Revision3.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK | Dry joint on CF socket.

## Revision 2

### Operator Name:

bill

### Time Stamp:

2005-09-05, 15:47:15

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 030
Batch_No | 7266

2D Barcode Value
30201300000057

Opto RX | Serial Number
--- | ---
1 | 380212
2 | 380211
3 | 380214
4 | 380213
5 | 380216
6 | 380218
7 | 380215
8 | 380217

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/057/BS_Files/BS_Ident_File_057_Revision2.txt
Boundary Scan 'Inter' Test | OK | Boundary Scan Clock TCK Frequency: 2MHz | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/057/BS_Files/BS_Inter_File_057_Revision2.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | Fail |

## Revision 1

### Operator Name:

brenda

### Time Stamp:

2005-08-25, 16:24:30

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 030
Batch_No | 7266

2D Barcode Value
30201300000057

Opto RX | Serial Number
--- | ---
1 | 380212
2 | 380211
3 | 380214
4 | 380213
5 | 380216
6 | 380218
7 | 380215
8 | 380217

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /
Boundary Scan 'Inter' Test | Fail |  | /

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Unattempted |
Power On In System Test Crate | Unattempted |
Program VME PROM | Unattempted |
Reboot PC3205, Check Flashing LEDs | Unattempted |

## Revision 0

### Operator Name:

Brenda

### Time Stamp:

2005-08-25, 15:55:37

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 030
Batch_No | 7266

2D Barcode Value
30201300000057

Opto RX | Serial Number
--- | ---
1 | 380212
2 | 380211
3 | 380214
4 | 380213
5 | 380216
6 | 380218
7 | 380215
8 | 380217

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | Fail |  | /
Boundary Scan 'Inter' Test | Unattempted |  | /

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Unattempted |
Power On In System Test Crate | Unattempted |
Program VME PROM | Unattempted |
Reboot PC3205, Check Flashing LEDs | Unattempted |