# Manual FED Entries / Test Results

## Revision 3

### Operator Name:

bill

### Time Stamp:

2005-09-08, 13:10:35

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 015
Batch_No | 7266

2D Barcode Value
30201300000078

Opto RX | Serial Number
--- | ---
1 | 370366
2 | 370367
3 | 370368
4 | 370369
5 | 370371
6 | 370370
7 | 370372
8 | 370373

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/078/BS_Files/BS_Ident_File_078_Revision3.txt
Boundary Scan 'Inter' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/078/BS_Files/BS_Inter_File_078_Revision3.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 2

### Operator Name:

bill

### Time Stamp:

2005-09-02, 04:13:54

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 015
Batch_No | 7266

2D Barcode Value
30201300000076

Opto RX | Serial Number
--- | ---
1 | 370366
2 | 370367
3 | 370368
4 | 370369
5 | 370371
6 | 370370
7 | 370372
8 | 370373

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/078/BS_Files/BS_Ident_File_078_Revision2.txt
Boundary Scan 'Inter' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/078/BS_Files/BS_Inter_File_078_Revision2.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 1

### Operator Name:

bill

### Time Stamp:

2005-09-01, 04:14:08

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 015
Batch_No | 7266

2D Barcode Value
30201300000076

Opto RX | Serial Number
--- | ---
1 | 370366
2 | 370367
3 | 370368
4 | 370369
5 | 370371
6 | 370370
7 | 370372
8 | 370373

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/078/BS_Files/BS_Ident_File_078_Revision1.txt
Boundary Scan 'Inter' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/078/BS_Files/BS_Inter_File_078_Revision1.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |

## Revision 0

### Operator Name:

paul

### Time Stamp:

2005-08-30, 13:06:19

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 015
Batch_No | 7266

2D Barcode Value
30201300000076

Opto RX | Serial Number
--- | ---
1 | 370366
2 | 370367
3 | 370368
4 | 370369
5 | 370371
6 | 370370
7 | 370372
8 | 370373

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | Unattempted |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/078/BS_Files/BS_Ident_File_078_Revision0.txt
Boundary Scan 'Inter' Test | Fail |  | /

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Unattempted |
Power On In System Test Crate | Unattempted |
Program VME PROM | Unattempted |
Reboot PC3205, Check Flashing LEDs | Unattempted |