# Manual FED Entries / Test Results

## Revision 0

### Operator Name:

noel

### Time Stamp:

2006-05-19, 11:01:02

### Pre Boundary Scan:

Action | Status | Comments
--- | --- | ---
Visual Inspection | OK |
Power Supply Short Circuit Check | OK |
Fit Serial No. To PCB | Done |
Fit Front Panel Serial No. Label | Done |
Enter Manufacturer Reference Numbers | Done
Attach 2D Barcode | Done
Enter Opto RX Serial Numbers | Done
Check Insertion In Boundary Scan Crate | OK |
Check Card Power Up | OK |

Manufacturers Reference No. | Value
--- | ---
PCB_No | 0471
Batch_No | 7573

2D Barcode Value
30201300000513

Opto RX | Serial Number
--- | ---
1 | 350443
2 | 350441
3 | 350442
4 | 350440
5 | 350439
6 | 350438
7 | 350403
8 | 350429

### Boundary Scan:

Action | Status | Comments | Boundary Scan File
--- | --- | --- | ---
Boundary Scan 'Ident' Test | OK | ref ic108 new ident | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/513/BS_Files/BS_Ident_File_513_Revision0.txt
Boundary Scan 'Inter' Test | OK |  | /home/fed/FedIndustryTest/LabVIEW_Executable/TestReports/513/BS_Files/BS_Inter_File_513_Revision0.txt

### Post Boundary Scan:

Action | Status | Comments
--- | --- | ---
Plug In Compact Flash Card | Done |
Power On In System Test Crate | Done |
Program VME PROM | OK |
Reboot PC3205, Check Flashing LEDs | OK |